**Publications: Salah JELLALI**

Localisation:

Laboratoire Eaux Usées et Environnement, puis sous rubrique personnel puis sous rubrique Publications puis sous rubrique année

|  |  |
| --- | --- |
| **Reference** | **Web link** |
| **2019** | |
| Dutournié, P., Jeguirim, M., Khiari, B., Goddard, M. L., **Jellali, S.** (2019). Olive Mill Wastewater: From a Pollutant to Green Fuels, Agricultural Water Source, and Bio-Fertilizer. Part 2: Water Recovery. Water, 11(4), 768. | <https://pubs.acs.org/doi/abs/10.1021/acssuschemeng.7b01786> |
| Ibn Ferjani, A., Jeguirim, M., **Jellali, S.,** Limousy, L., Courson, C., Thevenin, N., Ruidavets, L., Akrout, H., Audrey, A., Bennici, S. **(2019)**. The use of exhausted grape marc to produce biofuels and biofertilizers: Effect of pyrolysis temperatures on biochars properties. Renewable & Sustainable Energy Reviews, 107, 425-433 | <https://www.sciencedirect.com/science/article/pii/S1364032119301741> |
| Daly, I., **Jellali, S.**, Mehri, I., Reis, M.A.M., Freitas, E. B., Oehmen, A., Chatti, A. (2019): Phosphorus and ammonium removal characteristics from aqueous solutions by a newly isolated plant growth-promoting bacterium. Environmental technology, accepted in under press, https://doi.org/10.1080/09593330.2019.1575917 | <https://www.tandfonline.com/doi/abs/10.1080/09593330.2019.1575917?journalCode=tent20> |
| Ghazouani, M., Akrout, H., **Jellali, S.**, Bousselmi. L. (2019): Comparative study of electrochemical hybrid systems for the treatment of real wastewaters from agri-food activities*. Science of the Total Environment,* 647, 1651-1664. | <https://www.sciencedirect.com/science/article/pii/S0048969718329929> |
| **2018** | |
| Azzaz, A. A**.**, **Jellali, S.**, Bengharez, Z., Bousselmi, L., & Akrout, H. **(2018)**. Investigations on a dye desorption from modified biomass by using a low-cost eluent: hysteresis and mechanisms exploration. *International Journal of Environmental Science and Technology*. doi:10.1007/s13762-018-2171-3. | <https://link.springer.com/article/10.1007/s13762-018-2171-3> |
| Azzaz, A. A., **Jellali, S.**, Akrout, H., Assadi, Bousselmi, L. (2018) : Dynamic investigations on cationic dye desorption from chemically modified lignocellulosic material using a low-cost eluent: Dye recovery and anodic oxidation efficiencies of the desorbed solutions, *Journal of Cleaner Production*, 201, 28-38. | <https://www.sciencedirect.com/science/article/pii/S0959652618323540> |
| Mlayah, A., **Jellali, S.** (2018): Powdered marble wastes reuse for cadmium removal from aqueous solutions under dynamic conditions. *Environmental Engineering and Management Journal*, 17, 1139-1147 | <http://www.eemj.icpm.tuiasi.ro/pdfs/accepted/22_211_Mlayah_14.pdf> |
| Azzaz, A. A., Assadi, A. A., **Jellali, S.**, Bouzaza, A. Wolbert, D., Rtimi, S., Bousselmi, L. (2018): Discoloration of simulated textile effluent in continuous photoreactor using immobilized titanium dioxide: Effect of zinc and sodium chloride. *Journal of Photochemistry & Photobiology, A: Chemistry*, 358, 111-120. | <https://www.sciencedirect.com/science/article/abs/pii/S1010603017314119> |
| Haddad, K., **Jellali, S.**, Jeguirim, M., Ben Hassen Trabelsi, A., Limousy, L. (2018): Investigations on phosphorus recovery from aqueous solutions by biochars derived from magnesium-pretreated cypress sawdust. *Journal of Environmental Management*, 216, 305-314. | <https://www.sciencedirect.com/science/article/pii/S0301479717306011> |
| **2017** | |
| Haddad, K., Jeguirim, M., Jerbi, B., Chouchene, A., Dutournie, P., Thevenin, N., Ruidavets, L., **Jellali, S.**, Limousy, L. **(2017)**: Olive Mill Wastewater: From a Pollutant to Green Fuels, Agricultural Water Source and Biofertilizer, ACS *Sustainable Chemistry and Engineering*, *5* (10), 8988-8996. | <https://pubs.acs.org/doi/abs/10.1021/acssuschemeng.7b01786> |
| Azzaz, A.A., **Jellali,S.**, Souissi, R., Ergaieg,K., Bousselmi, L. (2017): Alkaline-treated sawdust as an effective material for cationic dye removal from textile effluents under dynamic conditions: breakthrough curve prediction and mechanism exploration. *Environmental Science and Pollution Research*. 24 (22), 18240-18256. | <https://link.springer.com/article/10.1007/s11356-017-9388-4> |
| Haddad, K., Jeguirim, M., **Jellali, S.**, Guizani, C., Delmotte, L., Bennici, S., Limousy, L. (2017): Combined NMR structural characterization and thermogravimetric analyses for the assessment of the AAEM effect during lignocellulosic biomass pyrolysis. *Energy*, 134, 10-23. | <https://www.sciencedirect.com/science/article/abs/pii/S0360544217310149> |
| **2016** | |
| Azzaz, A. A., **Jellali, S.**, Akrout, H., Assadi, A. A., Bousselmi, L. **(2016)**: Optimization of a cationic dye removal by a chemically modified agriculture by-product using response surface methodology: biomasses characterization and adsorption properties, *Environmental Science and Pollution Research,* 24 (11), 9831-9846. | <https://link.springer.com/article/10.1007/s11356-016-7698-6> |
| Ghazouani, M., Akrout, H., Jomaa, S., **Jellali, S.**, Bousselmi. L. (2016): Enhancing removal from highly concentrated synthetic wastewaters using bipolar Si/BDD cell: Optimization and mechanism study. *Journal of electroanalytical chemistry*, 783, 28-40. | <https://www.sciencedirect.com/science/article/pii/S1572665716305902> |
| **Jellali, S.**, Diamantopoulos, E., Haddad, K., Anane, M., Durner, W., Mlayah, A (2016) : Lead removal from aqueous solutions by raw sawdust and magnesium pretreated biochar: experimental investigations and numerical modelling. *Journal of Environmental Management*, 180, 439-449. | <https://www.sciencedirect.com/science/article/pii/S0301479716303103> |
| Azzaz, A. A., **Jellali, S.**, Assadi, A. A., Bousselmi, L. (2016): Chemical treatment of orange tree sawdust for a cationic dye enhancement removal from aqueous solutions: kinetic, equilibrium and thermodynamic studies, *Desalination and water treatment*, 57(46), 22107-22119. | <https://www.tandfonline.com/doi/abs/10.1080/19443994.2015.1103313> |
| **2015** | |
| Gdoura, K., Anane, M., **Jellali, S.** **(2015)**: Geospatial and multi-criteria analysis to rank suitable sites of shallow aquifer recharge with reclaimed water: Application to Nabeul - Hammamet shallow groundwater. *Resources, Conservation & Recycling*, 104, 19-30. | <https://www.sciencedirect.com/science/article/pii/S0921344915300811> |
| Mlayah, A. **Jellali, S.** (2015): Study of continuous lead removal from aqueous solutions by marble wastes: efficiencies and mechanisms. *International journal of environmental science and technology*. 12, 2965–2978. | <http://www.bioline.org.br/pdf?st15279> |
| Haddad, K., **Jellali, S.**, Jaouadi, S., Benltifa, M., Mlayah, A., Hamzaoui, A. H. (2015): Raw and treated marble wastes reuse as a low cost material for phosphorus removal from aqueous solutions: efficiencies and mechanisms. *Comptes rendus chimie*, 18, 75–87. | <https://www.sciencedirect.com/science/article/pii/S1631074814001908> |
| Akrout, H. **Jellali, S.**, Bousselmi, L. (2015) : Enhancement of methylene blue removal by anodic oxidation using BDD electrode combined with adsorption onto sawdust, *Comptes rendus chimie*, 18, 110-120 | <https://www.sciencedirect.com/science/article/pii/S1631074814002203> |